<!DOCTYPE html PUBLIC "-//W3C//DTD XHTML 1.0 Transitional//EN" "http://www.w3.org/TR/xhtml1/DTD/xhtml1-transitional.dtd">

<!-- saved from url=(0014)about:internet -->
<html xmlns="http://www.w3.org/1999/xhtml" xml:lang="en" lang="en">
  <head>
    <meta http-equiv="Content-Type" content="text/html; charset=UTF-8" />
    <meta http-equiv="Content-Style-Type" content="text/css" />
    <meta name="GENERATOR" content="Quadralay WebWorks AutoMap 2003 Platinum Edition Client for FrameMaker 8.6.6597.0" />
    <meta name="TEMPLATEBASE" content="emwebh8-1-17" />
    <meta name="LASTUPDATED" content="08/01/13 14:45:16" />
    <title>FC Interfaces ELP </title>
    <!-- Copyright 2010-2013, Cisco Systems, Inc. All rights reserved. -->

    <link rel="StyleSheet" href="document.css" type="text/css" />
    <link rel="StyleSheet" href="catalog.css" type="text/css" />


<script> 
    var is_chrome = navigator.userAgent.toLowerCase().indexOf('chrome') > -1; 
   
    if(is_chrome){document.domain=document.domain}
   </script>
    <script type="text/javascript" language="JavaScript1.2" src="expand.js"></script>
    <script type="text/javascript" language="JavaScript1.2" src="page.js"></script>

    <script type="text/javascript" language="JavaScript1.2">
     <!--
      function  WWNoOp() {}
      function  WWNoValue() { return ""; }

      var  VarDropDown;

      if (typeof(HTMLHelp_Object) != "undefined")
      {
        VarDropDown = new WWDropDown_Object();
      }
      else
      {
        VarDropDown = new Object();
        VarDropDown.fAnchorOpen  = WWNoOp;
        VarDropDown.fAnchorClose = WWNoOp;
        VarDropDown.fDIVOpen  = WWNoOp;
        VarDropDown.fDIVClose = WWNoOp;
      }
     // -->
    </script>

  
<SCRIPT language="javascript">
<!--
  self.document.write("<link href='"+top.relPath+"shared/style.css' rel='stylesheet' type='text/css'>");
  myid=53;
  self.document.write("<script type='text/javascript' language='JavaScript' src='"+top.relPath+"shared/con_utils.js'></scr"+"ipt>");
//-->
</SCRIPT>
</head>

  <body onload="highlightSearchTerms();" bgcolor="#ffffff">

    
    <blockquote>
    <a name="top"></a>

    
    


<a name="wp1044637"> </a><h1 class="pTitle">



FC Interfaces ELP

</h1>
<a name="wp1044699"> </a><p class="pBodyRelative">
</p><div>
<table border="2" cellpadding="2" id="wp1044640table1044638">
  <caption></caption>
  <tr bgcolor="#CCCCCC" align="left" valign="middle">    <th><a name="wp1044640"> </a><p class="pCellHeading">
Field 

</p>
</th>
    <th><a name="wp1044642"> </a><p class="pCellHeading">
Description 

</p>
</th>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1044644"> </a><p class="pBody">
Neighbor Port

</p>
</td>
    <td><a name="wp1044646"> </a><p class="pBody">
The port world wide name of the peer Interconnect_Port. 

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1044648"> </a><p class="pBody">
Neighbor Switch

</p>
</td>
    <td><a name="wp1044650"> </a><p class="pBody">
The node world wide name of the peer Node. 

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1044652"> </a><p class="pBody">
BBCredit Rx

</p>
</td>
    <td><a name="wp1044654"> </a><p class="pBody">
The maximum number of receive buffers available for holding Class 2, 
Class 3, Class F frames received from the peer Interconnect_Port. It is 
for buffer-to-buffer flow control in the incoming direction from the peer 
Interconnect_Port to local Interconnect_Port. <br />
The buffer-to-buffer flow control mechanism is indicated in the 
respective BbCreditModel. 

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1044656"> </a><p class="pBody">
BBCredit Tx

</p>
</td>
    <td><a name="wp1044658"> </a><p class="pBody">
The total number of buffers available for holding Class 2, Class 3, Class 
F frames to be transmitted to the peer Interconnect_Port. It is for 
buffer-to-buffer flow control in the direction from the local 
Interconnect_Port to peer Interconnect_Port. <br />
The buffer-to-buffer flow control mechanism is indicated in the 
corresponding BbCreditModel. 

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1044660"> </a><p class="pBody">
CoS

</p>
</td>
    <td><a name="wp1044662"> </a><p class="pBody">
The classes of services that the peer Interconnect_Port has requested the 
local Interconnect_Port to support and the local Interconnect_Port has 
granted the request. 

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1044664"> </a><p class="pBody">
Class2 SeqDeliv

</p>
</td>
    <td><a name="wp1044666"> </a><p class="pBody">
Whether the local Interconnect_Port has agreed to support Class 2 
sequential delivery during the Exchange Link Parameters Switch Fabric 
Internal Link Service request. This is meaningful only if Class 2 service 
has been agreed. 

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1044668"> </a><p class="pBody">
Class2 RxDataSize

</p>
</td>
    <td><a name="wp1044670"> </a><p class="pBody">
 The Class 2 Receive Data Field Size of the peer Interconnect_Port. 
Specifies the largest Data Field Size for an FT_1 frame that can be 
received by the Interconnect_Port. This is meaningful only if Class 2 
service has been agreed. 

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1044672"> </a><p class="pBody">
Class3 SeqDeliv

</p>
</td>
    <td><a name="wp1044674"> </a><p class="pBody">
Whether the local Interconnect_Port has agreed to support Class 3 
sequential delivery during the Exchange Link Parameters Switch Fabric 
Internal Link Service request. This is meaningful only if Class 3 service 
has been agreed. 

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1044676"> </a><p class="pBody">
Class3 RxDataSize

</p>
</td>
    <td><a name="wp1044678"> </a><p class="pBody">
The Class 3 Receive Data Field Size of the peer Interconnect_Port. 
Specifies the largest Data Field Size for an FT_1 frame that can be 
received by the Interconnect_Port. This is meaningful only if Class 3 
service has been agreed. 

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1044680"> </a><p class="pBody">
ClassF X_ID

</p>
</td>
    <td><a name="wp1044682"> </a><p class="pBody">
When true indicates that the peer Interconnect_Port supplying this 
parameter requires that an interlock be used during X_ID assignment in 
Class F. This is meaningful only if Class F service has been agreed. 

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1044684"> </a><p class="pBody">
ClassF RxDataSize

</p>
</td>
    <td><a name="wp1044686"> </a><p class="pBody">
The Class F Receive Data Field Size of the peer Interconnect_Port. 
Class F service is always agreed between two Interconnect_Ports. 
Specifies the largest Data Field Size for an FT_1 frame that can be 
received by the Interconnect_Port. 

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1044688"> </a><p class="pBody">
ClassF ConSeq

</p>
</td>
    <td><a name="wp1044690"> </a><p class="pBody">
The number of sequence status blocks provided by the 
Interconnect_Port supplying the parameters for tracking the progress of 
a sequence as a sequence recipient. The maximum number of concurrent 
sequences that can be specified is 255. A value of N/A in this field is 
reserved. 

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1044692"> </a><p class="pBody">
ClassF EECredit

</p>
</td>
    <td><a name="wp1044694"> </a><p class="pBody">
The maximum number of Class F data frames which can be transmitted 
by an Interconnect_Port without receipt of accompanying ACK or 
Link_Response frames. The minimum value of end-to-end credit is one. 
The end-to-end credit field specified is associated with the number of 
buffers available for holding the Data_Field of a Class F frame and 
processing the contents of that Data_Field by the Interconnect_Port 
supplying the parameters. 

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1044696"> </a><p class="pBody">
ClassF OpenSeq

</p>
</td>
    <td><a name="wp1044698"> </a><p class="pBody">
The open sequences per exchange shall specify the maximum number of 
sequences that can be open at one time at the recipient between a pair of 
Interconnect_Ports for one exchange. This value is used for exchange 
and sequence tracking.

</p>
</td>
</tr>
</table>
</div>
<p class="pBodyRelative">
</p>
<hr /><br><p class="pBody">Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.</p> 

    </blockquote>

  </body>
</html>
