> # Configuring Fibre Channel Using DCNM-SAN

> ## Detailed Steps

> To configure a Fibre Channel using DCNM-SAN, follow these steps:

> 1. Expand End Devices and then select SSM Features in the Physical Attributes pane.

> You see the Intelligent Storage Services configuration, showing the FCWA tab in the Information pane.

> 2. Click Create Row in the Information pane to create a SCSI flow or click a row in the FCWA table to modify an existing SCSI flow.

> You see the FC Write Acceleration dialog box.

> 3. Select the initiator and target WWNs and VSAN IDs and check the WriteAcc check box to enable Fibre Channel Write Acceleration on this SCSI flow.
> 4. (Optional) Enable SCSI flow statistics on this SCSI flow by checking the Enable Statistics check box.
> 5. (Optional) Change the BufCount value to set the number of 2K buffers used by the SCSI target.
> 6. Click Create to create this SCSI flow.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.