## Images and Configuration

This feature enables you to specify the servers & credential used to access the device images and the uploaded or DCNM generated/published device configuration. The server containing the images could be different from the one containing the configurations. If the same server contains both images and configurations, you must provide the server IP address and credentials twice for each server, if the directories holding images and configuration files are different. By default, DCNM server will be the default image and configuration server.

Copy Kickstart and system images into the repository prior to defining POAP definitions for devices. If the DCNM is the image repository, copy the image files into /var/lib/dcnm/ directory.

• Add Image or Configuration Server URL

• Editing an Image or Configuration Server URL

• Deleting an Image or Configuration Server URL