> # Replacing a Server on the Same Port

> ## Detailed Steps

> To replace a failed server with a new server on the same port, follow these steps:

> 1. In the DCNM-SAN window, select Tools > NPV > FlexAttach Replace Server.

> The Replace Failed Server window is displayed.

> 2. In the Replace Server Wizard, click the On Same Port radio button.
> 3. Click Next.

> The Choose Failed Port window is displayed.

> 4. In the Choose Failed Port selection window, from the Select a switch drop-down list, select the switch.
> 5. From the list of interfaces displayed, select the port on which the server needs to be replaced.
> 6. Click Next.

> The Server WWN window is displayed.

> 7. In the Server WWN window, enter the existing FlexAttach server virtual port WWN that needs to be replaced, and the new server physical port WWN.
> 8. Click Finish to complete the FlexAttach configuration for the new server.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.