> # FCIP Tunnels

> Field | Description
> --- | ---
> Interface | This identifies the interface on this FCIP device to which this link pertains.
> Attached | The interface on which this FCIP link was initiated.
> B Port Enable | If true, the B port mode is enabled on the local FCIP link.
> B Port KeepAlive | If true, a message is sent in response to a (Fibre Channel) ELS Echo frame received from the peer. Some B Port implementations use ELS Echo request/response frames as link keep alive.
> Remote IP Address | The Internet address for the remote FCIP entity.
> Remote TCP Port | The remote TCP port to which the local FCIP entity will connect if and when it initiates a TCP connection setup for this link.
> Spc Frames Enable | If true, the TCP active opener initiates FCIP special frames and the TCP passive opener responds to the FCIP special frames. If it is set to false, the FCIP special frames are neither generated nor responded to.
> Spc Frames RemoteWWN | The world wide name of the remote FC fabric entity. If this is a zero length string then this link would accept connections from any remote entity. If a WWN is specified then this link would accept connections from a remote entity with this WWN.
> Spc Frames Remote Profile Id | The remote FCIP entity's identifier.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.