<!DOCTYPE html PUBLIC "-//W3C//DTD XHTML 1.0 Transitional//EN" "http://www.w3.org/TR/xhtml1/DTD/xhtml1-transitional.dtd">

<!-- saved from url=(0014)about:internet -->
<html xmlns="http://www.w3.org/1999/xhtml" xml:lang="en" lang="en">
  <head>
    <meta http-equiv="Content-Type" content="text/html; charset=UTF-8" />
    <meta http-equiv="Content-Style-Type" content="text/css" />
    <meta name="GENERATOR" content="Quadralay WebWorks AutoMap 2003 Platinum Edition Client for FrameMaker 8.6.6597.0" />
    <meta name="TEMPLATEBASE" content="emwebh8-1-17" />
    <meta name="LASTUPDATED" content="08/01/13 14:48:06" />
    <title>Target Storage Device Requiring LUN Mapping Example </title>
    <!-- Copyright 2010-2013, Cisco Systems, Inc. All rights reserved. -->

    <link rel="StyleSheet" href="document.css" type="text/css" />
    <link rel="StyleSheet" href="catalog.css" type="text/css" />


<script> 
    var is_chrome = navigator.userAgent.toLowerCase().indexOf('chrome') > -1; 
   
    if(is_chrome){document.domain=document.domain}
   </script>
    <script type="text/javascript" language="JavaScript1.2" src="expand.js"></script>
    <script type="text/javascript" language="JavaScript1.2" src="page.js"></script>

    <script type="text/javascript" language="JavaScript1.2">
     <!--
      function  WWNoOp() {}
      function  WWNoValue() { return ""; }

      var  VarDropDown;

      if (typeof(HTMLHelp_Object) != "undefined")
      {
        VarDropDown = new WWDropDown_Object();
      }
      else
      {
        VarDropDown = new Object();
        VarDropDown.fAnchorOpen  = WWNoOp;
        VarDropDown.fAnchorClose = WWNoOp;
        VarDropDown.fDIVOpen  = WWNoOp;
        VarDropDown.fDIVClose = WWNoOp;
      }
     // -->
    </script>

  
<SCRIPT language="javascript">
<!--
  self.document.write("<link href='"+top.relPath+"shared/style.css' rel='stylesheet' type='text/css'>");
  myid=2016;
  self.document.write("<script type='text/javascript' language='JavaScript' src='"+top.relPath+"shared/con_utils.js'></scr"+"ipt>");
//-->
</SCRIPT>
</head>

  <body onload="highlightSearchTerms();" bgcolor="#ffffff">

    
    <blockquote>
    <a name="top"></a>

    
    


<a name="wp1199718"> </a><h1 class="pTitle">
Target Storage Device Requiring LUN Mapping Example

</h1>
<a name="wp1199722"> </a><p class="pBody">
This example scenario 2 assumes the following configuration:

</p>
<div class="pSmartList1"><ul class="pSmartList1">
<a name="wp1199723"> </a><li class="pSmartList1">Access control is based on Fibre Channel zoning.
</li>
<a name="wp1199724"> </a><li class="pSmartList1">There is target-based LUN mapping or LUN masking.
</li>
<a name="wp1199725"> </a><li class="pSmartList1">There is no iSCSI authentication (none).
</li>
<a name="wp1199726"> </a><li class="pSmartList1">The iSCSI initiator is assigned to different VSANs.
</li>
</ul></div>
<a name="wp1199733"> </a><h2 class="pHeading2">
Detailed Steps
</h2>
<a name="wp1337940"> </a><p class="pBody">
To configure this example, follow these steps:

</p>
<div class="pSmartList1"><ol type="1" class="pSmartList1">
<a name="wp1337942"> </a><li class="pSmartList1">Configure null authentication for all iSCSI hosts. 
</li>
<div class="pSmartList2"><ol type="a" class="pSmartList2">
<a name="wp1337943"> </a><li class="pSmartList2">In Cisco DCNM-SAN, choose <b style="font-weight: bold" class="cBold">End Devices </b><span style="font-weight: bold">&gt; </span><b style="font-weight: bold" class="cBold">iSCSI</b><span style="font-weight: bold"> </span>in the Physical Attributes pane.</li>
<a name="wp1337944"> </a><li class="pSmartList2">Select <b class="cBold">none </b>from the AuthMethod drop-down menu in the Information pane.</li>
<a name="wp1337945"> </a><li class="pSmartList2">Click the <b style="font-weight: bold" class="cBold">Apply Changes</b><span style="font-weight: bold"> </span>icon.</li>
</ol></div>
<a name="wp1337946"> </a><li class="pSmartList1">Configure iSCSI to dynamically import all Fibre Channel targets into the iSCSI SAN using 
auto-generated iSCSI target names.
</li>
<div class="pSmartList2"><ol type="a" class="pSmartList2">
<a name="wp1337947"> </a><li class="pSmartList2">In Device Manager, click <b style="font-weight: bold" class="cBold">IP</b><span style="font-weight: bold"> &gt; </span><b class="cBold">iSCSI.</b></li>
<a name="wp1337948"> </a><li class="pSmartList2">Click the<b style="font-weight: bold" class="cBold"> Targets</b><span style="font-weight: bold"> </span>tab. </li>
<a name="wp1337949"> </a><li class="pSmartList2">Check the <b class="cBold">Dynamically Import FC Targets</b> check box.</li>
<a name="wp1337950"> </a><li class="pSmartList2">Click <b class="cBold">Apply</b>.</li>
</ol></div>
<a name="wp1337951"> </a><li class="pSmartList1">Configure the Gigabit Ethernet interface in slot 7 port 1 with an IPv4 address and enable the interface.
</li>
<div class="pSmartList2"><ol type="a" class="pSmartList2">
<a name="wp1337952"> </a><li class="pSmartList2">In Cisco DCNM-SAN, choose <b style="font-weight: bold" class="cBold">Switches</b><span style="font-weight: bold"> &gt; </span><b style="font-weight: bold" class="cBold">Interfaces</b><span style="font-weight: bold"> &gt; </span><b style="font-weight: bold" class="cBold">Gigabit Ethernet</b><span style="font-weight: bold"> </span>in the Physical Attributes pane.</li>
<a name="wp1337953"> </a><li class="pSmartList2">Select the<span style="font-weight: bold"> </span><b class="cBold">IP Address</b> tab in the Information pane and click <b class="cBold">Create Row</b>.</li>
<a name="wp1337954"> </a><li class="pSmartList2">Set the IP address and subnet mask for the Gigabit Ethernet interface in slot 7 port 1.</li>
<a name="wp1337955"> </a><li class="pSmartList2">Click <b style="font-weight: bold" class="cBold">Create</b><span style="font-weight: bold">.</span></li>
<a name="wp1337956"> </a><li class="pSmartList2">Click the <b class="cBold">General </b>tab and select <b class="cBold">up</b> from the Admin drop-down menu for the Gigabit Ethernet interface in slot 7 port 1.</li>
<a name="wp1337957"> </a><li class="pSmartList2">Click the <b style="font-weight: bold" class="cBold">Apply Changes</b><span style="font-weight: bold"> </span>icon.</li>
</ol></div>
<a name="wp1337958"> </a><li class="pSmartList1">Configure the iSCSI interface in slot 7 port 1 to identify all dynamic iSCSI initiators by their IP address 
and enable the interface.
</li>
<div class="pSmartList2"><ol type="a" class="pSmartList2">
<a name="wp1337959"> </a><li class="pSmartList2">In Cisco DCNM-SAN, choose <b style="font-weight: bold" class="cBold">Switches</b><span style="font-weight: bold"> &gt; </span><b style="font-weight: bold" class="cBold">Interfaces </b><span style="font-weight: bold">&gt; </span><b class="cBold">FC Logical </b>in the Physical Attributes pane.</li>
<a name="wp1337960"> </a><li class="pSmartList2">Select the<span style="font-weight: bold"> </span><b style="font-weight: bold" class="cBold">iSCSI</b><span style="font-weight: bold"> </span>tab in the Information pane.</li>
<a name="wp1337961"> </a><li class="pSmartList2">Select <b class="cBold">ipaddress</b> from the Initiator ID Mode drop-down menu and click the <b class="cBold">Apply Changes</b> icon.</li>
<a name="wp1337962"> </a><li class="pSmartList2">In Device Manager, choose<span style="font-weight: bold"> </span><b style="font-weight: bold" class="cBold">Interfaces </b><span style="font-weight: bold">&gt; </span><b class="cBold">Ethernet and iSCSI</b>.</li>
<a name="wp1337963"> </a><li class="pSmartList2">Click the<b class="cBold"> iSCSI</b> tab.</li>
<a name="wp1337964"> </a><li class="pSmartList2">Select <b class="cBold">up </b>from the Admin drop-down menu for the iSCSI interface in slot 7 port 1.</li>
<a name="wp1337965"> </a><li class="pSmartList2">Click <b class="cBold">Apply</b>.</li>
</ol></div>
<a name="wp1337966"> </a><li class="pSmartList1">Configure the Gigabit Ethernet interface in slot 7 port 5 with the IPv4 address and enable the interface.
</li>
<div class="pSmartList2"><ol type="a" class="pSmartList2">
<a name="wp1337967"> </a><li class="pSmartList2">In Cisco DCNM-SAN, choose <b style="font-weight: bold" class="cBold">Switches</b><span style="font-weight: bold"> &gt; </span><b style="font-weight: bold" class="cBold">Interfaces </b><span style="font-weight: bold">&gt; </span><b style="font-weight: bold" class="cBold">Gigabit Ethernet</b><span style="font-weight: bold"> </span>in the Physical Attributes pane.</li>
<a name="wp1337968"> </a><li class="pSmartList2">Click the<span style="font-weight: bold"> </span><b class="cBold">IP Address</b> tab in the Information pane and click <b class="cBold">Create Row</b>.</li>
<a name="wp1337969"> </a><li class="pSmartList2">Set the IP address and subnet mask for the Gigabit Ethernet interface in slot 7 port 5.</li>
<a name="wp1337970"> </a><li class="pSmartList2">Click <b style="font-weight: bold" class="cBold">Create</b><span style="font-weight: bold">.</span></li>
<a name="wp1337971"> </a><li class="pSmartList2">Select the <b class="cBold">General</b> tab and select <b class="cBold">up </b>from the Admin drop-down menu for the Gigabit Ethernet interface in slot 7 port 5.</li>
<a name="wp1337972"> </a><li class="pSmartList2">Click the <b class="cBold">Apply Changes </b>icon.</li>
</ol></div>
<a name="wp1337973"> </a><li class="pSmartList1">Configure the iSCSI interface in slot 7 port 5 to identify all dynamic iSCSI initiators by IP address and 
enable the interface.
</li>
<div class="pSmartList2"><ol type="a" class="pSmartList2">
<a name="wp1337974"> </a><li class="pSmartList2">In Cisco DCNM-SAN, choose <b style="font-weight: bold" class="cBold">Switches</b><span style="font-weight: bold"> &gt; </span><b style="font-weight: bold" class="cBold">Interfaces</b><span style="font-weight: bold"> &gt;</span><b class="cBold"> FC Logical </b>in the Physical Attributes pane.</li>
<a name="wp1337975"> </a><li class="pSmartList2">Click the<b style="font-weight: bold" class="cBold"> iSCSI</b><span style="font-weight: bold"> </span>tab in the Information pane.</li>
<a name="wp1337976"> </a><li class="pSmartList2">Select <b class="cBold">ipaddress </b>from the Initiator ID Mode drop-down menu and click the<b class="cBold"> Apply Changes</b> icon.</li>
<a name="wp1337977"> </a><li class="pSmartList2">In Device Manager, choose<b style="font-weight: bold" class="cBold"> Interfaces </b><span style="font-weight: bold">&gt; </span><b class="cBold">Ethernet and iSCSI</b>.</li>
<a name="wp1337978"> </a><li class="pSmartList2">Click the<b class="cBold"> iSCSI</b> tab.</li>
<a name="wp1337979"> </a><li class="pSmartList2">Select <b class="cBold">up </b>from the Admin drop-down menu for the iSCSI interface in slot 7 port 5.</li>
<a name="wp1337980"> </a><li class="pSmartList2">Click <b class="cBold">Apply</b>.</li>
</ol></div>
<a name="wp1337981"> </a><li class="pSmartList1">Configure for static pWWN and nWWN for host 1.
</li>
<div class="pSmartList2"><ol type="a" class="pSmartList2">
<a name="wp1337982"> </a><li class="pSmartList2">In Device Manager, choose<span style="font-weight: bold"> </span><b style="font-weight: bold" class="cBold">IP</b><span style="font-weight: bold"> &gt; </span><b class="cBold">iSCSI</b>.</li>
<a name="wp1337983"> </a><li class="pSmartList2">Click the <b class="cBold">Initiators </b>tab.</li>
<a name="wp1337984"> </a><li class="pSmartList2">Check the<span style="font-weight: bold"> </span><b class="cBold">Node Address Persistent</b> and<span style="font-weight: bold"> </span><b class="cBold">Node Address System-assigned </b>check boxes the Host 1 iSCSI initiator.</li>
<a name="wp1337985"> </a><li class="pSmartList2">Click <b class="cBold">Apply</b>.</li>
</ol></div>
<a name="wp1337986"> </a><li class="pSmartList1">Configure for static pWWN for Host 2.
</li>
<div class="pSmartList2"><ol type="a" class="pSmartList2">
<a name="wp1337987"> </a><li class="pSmartList2">In Device Manager, Choose<b style="font-weight: bold" class="cBold"> IP</b><span style="font-weight: bold"> &gt; </span><b class="cBold">iSCSI</b>.</li>
<a name="wp1337988"> </a><li class="pSmartList2">Click the <b class="cBold">Initiators</b> tab.</li>
<a name="wp1337989"> </a><li class="pSmartList2">Right-click on the Host 2 iSCSI initiator and click Edit pWWN.</li>
<a name="wp1337990"> </a><li class="pSmartList2">Select<span style="font-weight: bold"> 1</span> from the System-assigned Num field and click <b class="cBold">Apply</b>.</li>
</ol></div>
<a name="wp1337991"> </a><li class="pSmartList1">View the configured WWNs. 
</li>
<a name="wp1337992"> </a><p class="pListNote1">
<strong>Note	&nbsp;&nbsp;&nbsp;</strong> The WWNs are assigned by the system. The initiators are members of different VSANs.

</p>
<div class="pSmartList2"><ol type="a" class="pSmartList2">
<a name="wp1337993"> </a><li class="pSmartList2">In Cisco DCNM-SAN, choose <b style="font-weight: bold" class="cBold">End Devices</b><span style="font-weight: bold"> &gt;</span><b style="font-weight: bold" class="cBold"> iSCSI</b><span style="font-weight: bold"> </span>in the Physical Attributes pane.</li>
<a name="wp1337994"> </a><li class="pSmartList2">Click the <b class="cBold">Initiators </b>tab.</li>
</ol></div>
<a name="wp1337995"> </a><li class="pSmartList1">Create a zone for Host 1 and the iSCSI target in VSAN 1.
</li>
<a name="wp1337996"> </a><p class="pListNote1">
<strong>Note	&nbsp;&nbsp;&nbsp;</strong> Use the IP address of the host in zone membership configuration because the iSCSI interface is 
configured to identify all hosts based on IP address.

</p>
<div class="pSmartList2"><ol type="a" class="pSmartList2">
<a name="wp1337997"> </a><li class="pSmartList2">In Cisco DCNM-SAN, choose <b style="font-weight: bold" class="cBold">Zones </b><span style="font-weight: bold">&gt; </span><b class="cBold">Edit Local Full Zone Database</b>.</li>
<a name="wp1337998"> </a><li class="pSmartList2">Select VSAN 1 from the VSAN drop-down menu in the Edit Local Full Zone Database dialog box.</li>
<a name="wp1337999"> </a><li class="pSmartList2">Select the<span style="font-weight: bold"> </span><b class="cBold">Zones </b>folder in the left navigation pane and click<b class="cBold"> Insert</b>.</li>
<a name="wp1338000"> </a><li class="pSmartList2">Set the Zone Name field to<b class="cBold"> iscsi-zone-1</b> and click <b style="font-weight: bold" class="cBold">OK</b><span style="font-weight: bold">.</span></li>
<a name="wp1338001"> </a><li class="pSmartList2">Select the iscsi-zone-1 folder in the left navigation pane and click <b class="cBold">Insert</b>.</li>
<a name="wp1338002"> </a><li class="pSmartList2">Set the ZoneBy radio button to<b style="font-weight: bold" class="cBold"> WWN</b><span style="font-weight: bold">.</span></li>
<a name="wp1338003"> </a><li class="pSmartList2">Set the Port WWN to the pWWN for the Fibre Channel target (that is, 21:00:00:20:37:6f:fd:97). and click <b class="cBold">Add</b>.</li>
<a name="wp1338004"> </a><li class="pSmartList2">Set the ZoneBy radio button to <b style="font-weight: bold" class="cBold">iSCSI IP Address/Subnet</b><span style="font-weight: bold">.</span></li>
<a name="wp1338005"> </a><li class="pSmartList2">Set the IP Address/Mask field to the IP Address for Host 1 iSCSI initiator (10.11.1.10) and click <b class="cBold">Add</b>.</li>
</ol></div>
<a name="wp1338006"> </a><p class="pListNote1">
<strong>Note	&nbsp;&nbsp;&nbsp;</strong> Fibre Channel storage for zone membership for the iSCSI initiator, either the iSCSI symbolic 
node name or the pWWN, can be used. In this case, the pWWN is persistent.

</p>
<a name="wp1338007"> </a><li class="pSmartList1">Create a zone set in VSAN 1 and activate it.
</li>
<div class="pSmartList2"><ol type="a" class="pSmartList2">
<a name="wp1338008"> </a><li class="pSmartList2">In Cisco DCNM-SAN, choose <b style="font-weight: bold" class="cBold">Zones</b><span style="font-weight: bold"> &gt; </span><b class="cBold">Edit Local Full Zone Database</b>.</li>
<a name="wp1338009"> </a><li class="pSmartList2">Select VSAN 1 from the VSAN drop-down menu in the Edit Local Full Zone Database dialog box.</li>
<a name="wp1338010"> </a><li class="pSmartList2">Select the<span style="font-weight: bold"> </span><b class="cBold">Zoneset </b>folder in the left navigation pane and click<b class="cBold"> Insert</b>.</li>
<a name="wp1338011"> </a><li class="pSmartList2">Set the Zoneset Name to <b class="cBold">zonset-iscsi-1</b> and click <b class="cBold">OK</b>.</li>
<a name="wp1338012"> </a><li class="pSmartList2">Click on the <b class="cBold">zoneset-iscsi-1</b> folder and click <b class="cBold">Insert</b>.</li>
<a name="wp1338013"> </a><li class="pSmartList2">Set the Zone Name field to<span style="font-weight: bold"> </span><b class="cBold">iscsi-zone-1 </b>and click <b style="font-weight: bold" class="cBold">OK</b><span style="font-weight: bold">.</span></li>
<a name="wp1338014"> </a><li class="pSmartList2">Click <b class="cBold">Activate</b> to activate the new zone set.</li>
<a name="wp1338015"> </a><li class="pSmartList2">Click<b class="cBold"> Continue Activation</b> to finish the activation.</li>
</ol></div>
<a name="wp1338016"> </a><li class="pSmartList1">Create a zone with host 2 and two Fibre Channel targets. 
</li>
<a name="wp1338017"> </a><p class="pListNote1">
<strong>Note	&nbsp;&nbsp;&nbsp;</strong> If the host is in VSAN 2, the Fibre Channel targets and zone must also be in VSAN 2.

</p>
<a name="wp1338018"> </a><p class="pListNote1">
<strong>Note	&nbsp;&nbsp;&nbsp;</strong> iSCSI interface is configured to identify all hosts based on node name.

</p>
<div class="pSmartList2"><ol type="a" class="pSmartList2">
<a name="wp1338019"> </a><li class="pSmartList2">In Cisco DCNM-SAN, choose <b style="font-weight: bold" class="cBold">Zones </b><span style="font-weight: bold">&gt; </span><b class="cBold">Edit Local Full Zone Database</b>.</li>
<a name="wp1338020"> </a><li class="pSmartList2">Select VSAN 2 from the VSAN drop-down menu in the Edit Local Full Zone Database dialog box.</li>
<a name="wp1338021"> </a><li class="pSmartList2">Select the<span style="font-weight: bold"> </span><b class="cBold">Zones </b>folder in the left navigation pane and click <b class="cBold">Insert</b>.</li>
<a name="wp1338022"> </a><li class="pSmartList2">Set the Zone Name field to<span style="font-weight: bold"> </span><b class="cBold">iscsi-zone-2</b> and click <b style="font-weight: bold" class="cBold">OK</b><span style="font-weight: bold">.</span></li>
<a name="wp1338023"> </a><li class="pSmartList2">Select the<span style="font-weight: bold"> </span><b class="cBold">iscsi-zone-2 </b>folder in the left navigation pane and click<b class="cBold"> Insert</b>.</li>
<a name="wp1338024"> </a><li class="pSmartList2">Set the ZoneBy radio button to<b style="font-weight: bold" class="cBold">WWN</b><span style="font-weight: bold">.</span></li>
<a name="wp1338025"> </a><li class="pSmartList2">Set the Port WWN to the pWWN for one of the Fibre Channel targets (for example, 21:00:00:20:37:6f:fe:5) and click <b class="cBold">Add</b>.</li>
<a name="wp1338026"> </a><li class="pSmartList2">Set the Port WWN to the pWWN for another of the Fibre Channel targets (for example, 21:00:00:20:37:a6:a6:5d) and click <b class="cBold">Add</b>.</li>
<a name="wp1338027"> </a><li class="pSmartList2">Set the ZoneBy radio button to <b style="font-weight: bold" class="cBold">iSCSI IP Address/Subnet</b><span style="font-weight: bold">.</span></li>
<a name="wp1338028"> </a><li class="pSmartList2">Set the IP Address/Mask field to the IP Address for Host 2 iSCSI initiator (10.15.1.11) and click <b class="cBold">Add</b>.</li>
</ol></div>
<a name="wp1338029"> </a><li class="pSmartList1">Create a zone set in VSAN 2 and activate it.
</li>
<div class="pSmartList2"><ol type="a" class="pSmartList2">
<a name="wp1338030"> </a><li class="pSmartList2">In Cisco DCNM-SAN, choose<b style="font-weight: bold" class="cBold"> Zones </b><span style="font-weight: bold">&gt; </span><b class="cBold">Edit Local Full Zone Database</b>.</li>
<a name="wp1338031"> </a><li class="pSmartList2">Select VSAN 2 from the VSAN drop-down menu in the Edit Local Full Zone Database dialog box.</li>
<a name="wp1338032"> </a><li class="pSmartList2">Select the<span style="font-weight: bold"> </span><b style="font-weight: bold" class="cBold">Zoneset</b><span style="font-weight: bold"> </span>folder in the left navigation pane and click <b class="cBold">Insert</b>.</li>
<a name="wp1338033"> </a><li class="pSmartList2">Set the Zoneset Name to <b class="cBold">zonset-iscsi-2</b> and click <b class="cBold">OK</b>.</li>
<a name="wp1338034"> </a><li class="pSmartList2">Click on the<b class="cBold"> zoneset-iscsi-2</b> folder and click <b class="cBold">Insert</b>.</li>
<a name="wp1338035"> </a><li class="pSmartList2">Set the Zone Name field to<span style="font-weight: bold"> </span><b class="cBold">iscsi-zone-2 </b>and click <b style="font-weight: bold" class="cBold">OK</b><span style="font-weight: bold">.</span></li>
<a name="wp1338036"> </a><li class="pSmartList2">Click <b class="cBold">Activate </b>to activate the new zone set.</li>
<a name="wp1338037"> </a><li class="pSmartList2">Click <b class="cBold">Continue Activation </b>to finish the activation.</li>
</ol></div>
<a name="wp1338038"> </a><li class="pSmartList1">Start the iSCSI clients on both hosts.
</li>
<a name="wp1338039"> </a><li class="pSmartList1">Show all the iSCSI sessions.
</li>
<div class="pSmartList2"><ol type="a" class="pSmartList2">
<a name="wp1338040"> </a><li class="pSmartList2">In Device Manager, choose<span style="font-weight: bold"> </span><b style="font-weight: bold" class="cBold">Interface</b><span style="font-weight: bold"> &gt; </span><b style="font-weight: bold" class="cBold">Monitor</b><span style="font-weight: bold"> &gt; </span><b style="font-weight: bold" class="cBold">Ethernet</b><span style="font-weight: bold"> </span>and select the<span style="font-weight: bold"> </span><b class="cBold">iSCSI connections </b>tab to show all the iSCSI sessions.</li>
<a name="wp1338041"> </a><li class="pSmartList2">In Device Manager, choose<span style="font-weight: bold"> </span><b style="font-weight: bold" class="cBold">IP</b><span style="font-weight: bold"> &gt; </span><b class="cBold">iSCSI</b> and select the <b class="cBold">Session Initiators </b>tab. </li>
<a name="wp1338042"> </a><li class="pSmartList2">Click <b style="font-weight: bold" class="cBold">Details</b><span style="font-weight: bold">.</span></li>
</ol></div>
<a name="wp1338043"> </a><li class="pSmartList1">In Cisco DCNM- SAN, choose <b style="font-weight: bold" class="cBold">End Devices </b><span style="font-weight: bold">&gt; </span><b class="cBold">iSCSI </b>in the Physical Attributes pane to verify the details 
of the two iSCSI initiators.
</li>
<a name="wp1338044"> </a><li class="pSmartList1">In Cisco DCNM-SAN, choose <b style="font-weight: bold" class="cBold">Zones </b><span style="font-weight: bold">&gt; E</span><b class="cBold">dit Local Full Zone Database </b>to view the active zone set. The 
iSCSI initiators&#39; FC IDs are resolved.
</li>
<a name="wp1338045"> </a><p class="pBodyRelative">

</p>
<a name="wp1338046"> </a><li class="pSmartList1">In Device Manager, choose<span style="font-weight: bold"> </span><b style="font-weight: bold" class="cBold">FC</b><span style="font-weight: bold"> &gt; </span><b style="font-weight: bold" class="cBold">Name Server</b><span style="font-weight: bold">. </span>The Fibre Channel name server shows the virtual N 
ports created for the iSCSI hosts.
</li>
<a name="wp1338047"> </a><li class="pSmartList1">In Device Manager, Choose<span style="font-weight: bold"> </span><b style="font-weight: bold" class="cBold">FC</b><span style="font-weight: bold"> &gt; </span><b class="cBold">Name Server.
</b></li>
<a name="wp1338048"> </a><li class="pSmartList1">Click the <b style="font-weight: bold" class="cBold">Advanced</b><span style="font-weight: bold"> </span>tab<span style="font-weight: bold">. </span>Verify the detailed output of the iSCSI initiator nodes in the Fibre Channel 
name server.
</li>
</ol></div>
<hr /><br><p class="pBody">Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.</p> 

    </blockquote>

  </body>
</html>
