> # Default Settings

> Table 12-7 lists the default settings for interface parameters.

> Table 12-7 Default Interface Parameters
> Parameters | Default
> --- | ---
> Interface mode | Auto
> Interface speed | Auto
> Administrative state | Shutdown (unless changed during initial setup)
> Trunk mode | On (unless changed during initial setup) on non-NPV and NPIV core switches. Off on NPV switches.
> Trunk-allowed VSANs or VF-IDs | 1 to 4093
> Interface VSAN | Default VSAN (1)
> Beacon mode | Off (disabled)
> EISL encapsulation | Disabled
> Data field size | 2112 bytes

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.