> # FCWA

> Field | Description
> --- | ---
> Flow Id | Represents the flow identifier.
> Init WWN | Represents the pWWN of the initiator in the flow.
> Init VSAN | The VSAN ID of the initiator on which the flow is configured.
> Target WWN | Represents the pWWN of the target in the flow.
> TargetVSAN | The VSAN ID of the target on which the flow is configured.
> WriteAcc | Specifies if write-acceleration feature is enabled for this flow. If set to true it is enabled. If set to false, it is disabled.
> BufCount | It specifies the number of buffers to be used for write-acceleration.
> Stats Enable | Specifies if the statistics gathering needs to be enabled for this flow. If set to true, then it is enabled. If it is set to false, then it is disabled.
> Stats Clear | Assists in clearing the statistics for this flow.
> Init Verification | The verification status of the initiator device corresponding to the SCSI flow.
> Init Module | The status of the linecard where the SCSI flow initiator device is located.
> Target Verification | The verification status of the target device corresponding to the SCSI flow.
> Target Module | The status of the linecard where the SCSI flow target device is located.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.