> # Disabling Restrictions on Oversubscription Ratios

> ## Prerequisites

> - Before disabling restrictions on oversubscription ratios, ensure that you have explicitly shut down shared ports.
> - This feature is only supported on 48-port and 24-port 4-Gbps, and 8-Gbps Fibre Channel switching modules.

> ## Detailed Steps

> To disable restrictions on oversubscription ratios on multiple 48-port or 24-port 4-Gbps, or any 8-Gbps Fibre Channel switching modules using DCNM-SAN, follow these steps:

> 1. Choose Switches > Hardware.
> 2. Click the Module Config tab. You see the Module Config dialog box.
> 3. From the RateModeOversubscriptionLimit drop-down list, select disabled for each module for which you want to disable restrictions on oversubscription ratios.
> 4. Click Apply to save the changes.

> To disable restrictions on oversubscription ratios on a single 48-port or 24-port 4-Gbps, or any 8-Gbps Fibre Channel switching module using Device Manager, follow these steps:

> 1. Right-click a module and select Configure.

> You see the Module dialog box.

> 2. Click the disabled radio button to disable restrictions on oversubscription ratios.
> 3. Click Apply to save the changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.