> # Copying FICON Configuration Files

> ## Detailed Steps

> To copy an existing FICON configuration file using Device Manager, follow these steps:

> 1. Choose FICON > VSANs.
> 2. Click the Files tab.

> You see the FICON VSANs dialog box.

> 3. Click Create to create a FICON configuration file.

> You see the Create FICON VSANs Files dialog box.

> 1. Select a VSAN ID for the FICON VSAN you want to configure.
> 2. Enter the file name and the description.
> 3. Click Create to create the file.
> 4. Click Copy to copy the file to a new file.
> 5. Click Apply to apply the FICON configuration file.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.