> # Enabling Call Home Fabric Distribution

> ## Detailed Steps

> To enable Call Home fabric distribution, follow these steps:

> 1. Select a switch in the Fabric pane.
> 2. Expand Events and select Call Home in the Physical Attributes pane.

> You see the Call Home information in the Information pane.

> 3. Click the CFS tab.

> You see the CFS information for Call Home.

> 4. Select a switch in the Information pane.
> 5. Select Enable from the drop-down list in the Admin column in the row for that switch.
> 6. Click the Apply Changes icon to commit the changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.