> # Clearing Previous Error Reports

> You can clear the error history for Fibre Channel interfaces, iSCSI interfaces, an entire module, or one particular test for an entire module. By clearing the history, you are directing the software to retest all failed components that were previously excluded from tests.

> If you previously enabled the failure-action option for a period of time (for example, one week) to prevent OHMS from taking any action when a failure is encountered and after that week you are now ready to start receiving these errors again, then you must clear the system health error status for each test.

> Tip The management port test cannot be run on a standby supervisor module.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.