> # Modifying an FCIP Link

> Once you have created FCIP links using the FCIP wizard, you may need to modify parameters for these links. This procedure includes modifying the FCIP profiles as well as the FCIP link parameters. Each Gigabit Ethernet interface can have three active FCIP links at one time.

> To modify an FCIP link, follow these steps on both switches:

> 1. Configure the Gigabit Ethernet interface.
> 2. Create an FCIP profile, and then assign the Gigabit Ethernet interface’s IP address to the profile.
> 3. Create an FCIP interface, and then assign the profile to the interface.
> 4. Configure the peer IP address for the FCIP interface.
> 5. Enable the interface.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.