> # Configuring Fibre Channel Analyzers Using SPAN

> ## Detailed Steps

> To configure Fibre Channel Analyzers using SPAN , follow these steps:

> 1. Configure SPAN on interface fc1/1 in the ingress (Rx) direction to send traffic on SD port fc2/1 using session 1.
> 2. Configure SPAN on interface fc1/1in the egress (Tx) direction to send traffic on SD port fc2/2 using session 2.
> 3. Physically connect fc2/1 to port 1 on the Fibre Channel analyzer.
> 4. Physically connect fc2/2 to port 2 on the Fibre Channel analyzer.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.