> # Editing FICON Configuration Files

> The configuration file submode allows you to create and edit FICON configuration files. If a specified file does not exist, it is created. Up to 16 files can be saved. Each file name is restricted to eight alphanumeric characters.

> Note To view the latest FICON information, you must click the Refresh button. See the "Automatically Saving the Running Configuration" topic.

> ## Detailed Steps

> To edit the contents of a specified FICON configuration file using Device Manager, follow these steps:

> 1. Choose FICON > VSANs.
> 2. Click the Files tab.

> You see the FICON VSANs dialog box.

> 3. Select a VSAN ID and then click Open to edit the FICON configuration file.
> 4. Select a VSAN ID and then click Delete to delete the FICON configuration file.
> 5. Click Apply to apply the changed FICON configuration file.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.