> # NP Link

> Field | Description
> --- | ---
> NPIV (core) | Name of the NPIV core switch.
> F port | The F port that is connected to the NPIV core switch
> NPV | Name of the NPV switch
> Speed | An estimate of the interface's current bandwidth in units of 1,000,000 bits per second. If this object reports a value of `n' then the speed of the interface is between `n-500,000' to `n+499,999'.
> Rx Util% | Received traffic Utilization %, total number of octets received on the interface over the speed configured on the interface, including framing characters
> Rx Bytes | The total number of octets received on the interface, including framing characters.
> Tx Util% | Recetransmittedived traffic Utilization %, total number of octets transmitted out of the interface over the speed configured on the interface, including framing characters.
> Tx Bytes | The total number of octets transmitted out of the interface, including framing characters.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.