> # Configuring Facility Severity Levels

> ## Detailed Steps

> To configure the severity level for a logging facility, follow these steps:

> 1. Expand Events and select SysLog in the Physical Attributes pane.

> In Device Manager, choose Logs > Syslog > Setup and click the Switch Logging tab in the Syslog dialog box.

> You see the switch information.

> 2. Check the check boxes where you want message logging to occur (ConsoleEnable, TerminalEnable, LineCardEnable).
> 3. Choose the message severity threshold from the Console Severity drop-down box for each switch in DCNM-SAN or click the appropriate message severity level radio button in Device Manager.
> 4. Click the Apply Changes icon in DCNM-SAN, or click Apply in Device Manager to save and apply your changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.