> # FC Interfaces Physical

> Field | Description
> --- | ---
> BeaconMode | If enabled, an interface LED is put into flashing mode for easy identification of a particular interface.
> ConnectorPresent | If true, there is a physical connector.
> ConnectorType | The module type of the port connector.
> TransmitterType | The technology of the port transceiver.
> Vendor | The connector unit vendor.
> PartNumber | The connector unit part number.
> Revision | The port revision of the connector unit.
> SerialNo | The serial number of the connector unit.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.