> # Configuring the multi-pid Option

> ## Detailed Steps

> To configure the multi-pid option, follow these steps:

> 1. Expand a fabric, expand a VSAN, and then select Advanced.

> You see the VSAN advanced configuration in the Information pane.

> 2. Click the RSCN Multi-PID tab.
> 3. Check the Enable check box.
> 4. Click Apply Changes to save these changes, or click Undo Changes to cancel any unsaved changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.