> # Presenting iSCSI Hosts as Virtual Fibre Channel Hosts

> The IPS module or MPS-14/2 module connects to the Fibre Channel storage devices on behalf of the iSCSI host to send commands and transfer data to and from the storage devices. These modules use a virtual Fibre Channel N port to access the Fibre Channel storage devices on behalf of the iSCSI host. iSCSI hosts are identified by either iSCSI qualified name (IQN) or IP address.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.