> # Information About Fibre Channel Write Acceleration

> Fibre Channel Write Acceleration minimizes application latency or reduces transactions per second over long distances. For synchronous data replication, Fibre Channel Write Acceleration increases the distance of replication or reduces effective latency to improve performance. With this feature you can also configure the buffer count and change the number of 2-KB buffers reserved on the target side DPP for a SCSI flow.

> To take advantage of this feature, both the initiator and target devices must be directly attached to an SSM.

> The Fibre Channel Write Acceleration feature also allows the configuration of the buffer count. You can change the number of 2-KB buffers reserved on the target side DPP for a SCSI flow.

> You can estimate the number of buffers to configure using the following formula:

> (Number of concurrent SCSI writes * size of SCSI writes in bytes) / FCP data frame size in bytes

> For example, HDS TrueCopy between HDS 9970s uses 1-KB FCP data frames. You perform an initial synchronization for a 16-LUN TrueCopy group with 15 tracks, or 768-KB per LUN, which requires approximately 16*(768*1024)/1024 or 12248 write buffers.

> Note The Fibre Channel Write Acceleration feature requires the Enterprise Package license installed on both the initiator and target switches.

> Note The initiator and target cannot connect to the same Cisco MDS switch. Fibre Channel Write Acceleration requires that the initiator and target must each connect to an SSM module installed on different Cisco MDS switches.

> Note Fibre Channel Write Acceleration can only be provisioned on the entire SSM, not a group of interfaces on the SSM.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.