> # Preferred Path Maps and Routes

> Field | Description
> --- | ---
> VSAN Id, Route Id | The VSAN ID of this FC route map. An arbitrary integer value that identifies a route in this FC route map.
> Map Active | Allows the activation/de-activation of all the routes within an FC route map. If true, then all the routes within this FC route map will be activated. If false, then all routes within this FC route map will be de-activated.
> Route Strict Preference | Allows changes to the way the preferred path selection logic will select the preferred path. Setting it to true makes the preferred path to select the outgoing interface strictly based on the preference set using the cPrefPathRMapSetIntfPref. When it is set to false, then the preferred path selection logic only performs selection only when the current outgoing interface goes down.
> Route Active | Allows the activation/de-activation of the route within an FC route map. If true, then the route will be activated. If false, then the route will be de-activated.
> RouteActive | Allows the activation/de-activation of the route within an FC route map. If true, then the route will be activated. If false, then the route will be de-activated.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.