> # Performing External Loopback Tests

> You can run manual loopback tests to identify hardware errors in the data path in the switching or services modules, and the control path in the supervisor modules. External loopback tests send and receive FC2 frames to and from the same port or between two ports.

> You need to connect a cable (or a plug) to loop the Rx port to the Tx port before running the test. If you are testing to and from the same port, you need a special loop cable. If you are testing to and from different ports, you can use a regular cable. This test is only available for Fibre Channel interfaces.

> Choose Interface > Diagnostics > External to perform an external loopback test from Device Manager.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.