> # Port Channels FC Interfaces

> Field | Description
> --- | ---
> PortVsan | VSAN to which this interface is statically assigned.
> Description | Alias name for the interface as specified by a network manager.
> Admin Mode | The port mode configured by the user. If the user configured the port as auto(1), then the port initialization scheme determines the mode of the port. In this case the user can look at OperMode to determine the current operating mode of port. Only auto(1) or ePort(4) is allowed.
> Oper Mode | The current operating mode of the port.
> Admin Speed | The port speed configured by the user.
> Oper Speed | The interface's current bandwidth per second.
> Admin Status | The desired state of the interface.
> Oper Status | The current operational state of the interface.
> FailureCause | The cause of current operational state of the port.
> LastChange | The time the interface entered its current operational state. If the current state was entered prior to the last re-initialization of the switch, then this is a zero or N/A value.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.