> # Enabling Call Home Function

> Once you have configured the contact information, you must enable the Call Home function.

> ## Detailed Steps

> To enable the Call Home function, follow these steps:

> 1. Select a switch in the Fabric pane.
> 2. Expand Events and select Call Home in the Physical Attributes pane.

> You see the Call Home information in the Information pane.

> 3. Click the Control tab.
> 4. Select a switch in the information pane.
> 5. Check the Duplicate Message Throttle check box.
> 6. Click the Apply Changes icon.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.