> # Cisco Fabric Services (CFS) Features

> Field | Description
> --- | ---
> Globally Enabled | Check this box to allow CFS on this switch to distribute feature configurations to other switches. Uncheck the box to prevent CFS from distributing the configuration to other switches.
> Feature | The name of the CFS-capable feature.
> Status | Status of the CFS-capable feature.
> Command | The action to be triggered for the feature. Actions include: noop - No operation. enable - Enable CFS distribution on the switch. disable - Disable CFS distribution on the switch. commit - Commit changes made since the session began. abort - Discard changes made, and close the session. clear - Discard changes made without closing the session.
> Type | The last CFS feature scope type used.
> VSAN Id | The ID of the VSAN on which this feature is running.
> RegionId | The distribution region ID that this CFS capable feature maps to. This region is required to be defined prior to its usage.
> View Config Changes As | Determines whether to view the changes as running or pending. A pending configuration exists until a Commit or Abort action is triggered for that feature. If the value is running then all subsequent configuration retrieval for this feature will be from the running configuration on the local device. If the value is pending then all subsequent configuration retrieval for this feature will be from the pending configuration on the local device.
> LastCommand | The last action performed on this feature.
> Result | Result of the action performed on the CFS-capable feature.
> Scope | The value of this object represents the attributes of a CFS-capable feature as registered with the CFS infrastructure. fcFabric - indicates that the CFS based distribution for a feature spans the entire FC (Fibre Channel) fabric ipNetwork - indicates that the CFS based distribution for a feature spans the entire IP network vsanScope - indicates that the CFS based distribution for a feature is done on per VSAN basis and restricted to a specific VSAN in a FC (Fibre Channel) fabric
> PendingConfOwnerAddr | The address of the device in the fabric where the pending configuration exists for the feature.
> Lock Owner Switch | The address of the device in the fabric where the pending configuration exists for the feature within this scope.
> Lock Owner UserName | The name of the device in the fabric where the pending configuration exists for the feature within this scope.
> Merge Status | The result of the last fabric merge for this feature within the context of the combination of scope type and scope value in the system. The following are the results: Success—Fabric merge completed successfully. InProgress—Fabric merge in progress. You may get this status when the local device that is a part of fabric engaged in the process of merging with another fabric. Failure—Fabric merge failed. Waiting—Waiting for existing merge to complete while the conflicts are being cleared. You may get this status when the local device that is a part of fabric waiting for any conflicts to be resolved before initiating a new instance of fabric merge. Other—None of the other values of this enumeration.
> Master | Select the CFS Master switch.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.