> # Interface Port Monitoring Link Errors

> The Monitor dialogs have special Monitor Dialog Controls.

> Field | Description
> --- | ---
> LinkFailures | The number of link failures detected by the FC-Port.
> SyncLosses | The number of loss of synchronization failures detected by the FC-Port.
> InvalidTxWords | The number of invalid transmission words detected by the FC-Port.
> AddressIdErrors | The number of address identifier errors detected by the FC-Port.
> PrimitiveSequenceProtocol Errors | Count of primitive sequence protocol errors detected at this port. This count is part of the Link Error Status Block (LESB). (FC-PH 29.8). Note, this is a Fibre Channel only stat.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.