> # Interface

> # Virtual Interface Groups

> The Bound Ethernet Interface field in the table can be modified. The remaining fields are for information only.

> Field | Description
> --- | ---
> Switch | Name of the switch hosting this virtual interface group (VIG).
> VIG Id | Virtual interface group identifier.
> Bound Eth Interface | Physical Ethernet interface associated with this VIG.
> Virtual Eth Interfaces | The virtual Ethernet interface bound to this VIG.
> Virtual FC Interfaces | The virtual FC interface bound to this VIG.
> Operational Status | The current operational state of the VIG.
> CreationTime | Date and time when the VIG was created.

> Note This table applies only to N5k switches running version less than 4.0(1a).

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.