> # VRRP Load Balancing Algorithm For Selecting Gigabit Ethernet Interfaces

> When the VRRP master receives an iSCSI session request from an initiator, it first checks for an existing mapping to one of the interfaces in that VRRP group. If such a mapping exists, the VRRP master redirects the initiator to that interface. If no such mapping exists, the VRRP master selects the least loaded interface and updates the selected interface’s load with the initiator’s iSLB metric (weight).

> Note The VRRP master interface is treated specially and it needs to take a lower load compared to the other interfaces. This is to account for the redirection work performed by the master interface for every session. A new initiator is assigned to the master interface only if the following is true for every other interface:
> VRRP backup interface load > [2 * VRRP master interface load + 1]

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.