> # Luke Line Card Bandwidth Reservation

> RateMode Config Macro | Description
> --- | ---
> Dedicated 10G on the following ports: Ports 1-8 Ports 9-16 Ports 17-24 Ports 25-32 Ports 33-40 Ports 41-48 | Allocates dedicated rate mode and admin speed of 10 Gbps on the specified ports.
> Unconfigure 10G on the following ports: Ports 1-8 Ports 9-16 Ports 17-24 Ports 25-32 Ports 33-40 Ports 41-48 | Reverts to default rate mode and admin speed on the specified ports. Transceiver frequencey is set to FC. This operation is disruptive.

> #

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.