> # Configuring DPVM with the DPVM Wizard

> ## Detailed Steps

> To use the DPVM Setup Wizard to set up dynamic port VSAN membership, follow these steps:

> 1. Click the DPVM Setup Wizard icon in the DCNM-SAN toolbar .

> You see the Select Master Switch page.

> 2. Click the switch you want to be the master switch. This switch controls the distribution of the DPVM database to other switches in the fabric.
> 3. Click Next.

> You see the AutoLearn Current End Devices page.

> 4. (Optional) Click the Create Configuration From Currently Logged In End Devices check box if you want to turn on autolearning.
> 5. Click Next.

> You see the Edit and Activate Configuration page.

> 6. Verify the current or autolearned configuration. Optionally, click Insert to add more entries into the DPVM config database.
> 7. Click Finish to update the DPVM config database, distribute the changes using CFS, and activate the database, or click Cancel to exit the DPVM Setup Wizard without saving changes.
> 8. Select the switch you want to be the master switch. This switch controls the distribution of the DPVM database to other switches in the fabric.
> 9. Click Next.

> You see the AutoLearn Current End Devices page.

> 10. (Optional) Check the Create Configuration From Currently Logged In End Devices check box if you want to enable autolearning.
> 11. Click Next.

> You see the Edit and Activate Configuration page.

> 12. Verify the current or autolearned configuration. Optionally, click Insert to add more entries into the DPVM config database.
> 13. Click Finish to update the DPVM config database, distribute the changes using CFS, and activate the database, or click Cancel to exit the DPVM Setup Wizard without saving changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.