BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1403
Time supervision of short register sign. alt. MFC/MFE outgoing

The command is used to determine the time for short time supervision between the digits at dialing, value 3 -255 seconds.

In case of MFC-signaling the time is used to supervise the MFC register signaling at an outgoing call.

In case of MFE-signaling the time is used to supervise the time a register is occupied by an outgoing call.

Timeout results in disconnection /blocking unless an open number has been received from the TCD-analysis, or in a switch to speech state if an open number has been dialed.

Note

For decadic pulsing this time must not be less than the time required by the BTU-board to transmit the digit.

(See commands 1401 Number of digits with long dial supervision and 1402 Time supervision of long register sign. alt. MFC/MFE outgoing) the relationship between the number of digits and the time for supervision is adapted for possible standard number series for the line.)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003