BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1413
Time supervision of answer at automatic incoming traffic

The command is used to state the supervision time for incoming calls between end of selection and answer before rerouting to an alternative answering position. The parameter shall only be used for lines of type direct in-dialing and automatic incoming tie lines.

Value 0-255 seconds. If the parameter is set to zero there will be no rerouting.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003