BusinessPhone Communication Platform 4.0
Facilities

## Saved External Number Redial

## Definition

Saved external number redial means that a dialled external number can be saved (stored) in a memory by depression of the key Save/Redial.

The saved number can later be retransmitted by depression of Save/Redial, when in idle state.

## Use

The function is very practicable when a called public network subscriber does not answer or is busy. It is then possible to make repeated attempts without having to dial the number manually on each occasion.

## Operation

### BASIC Telephones

#### Save number

An extension saves a dialled number as follows:

1. Press pre-programmed Save/Redial-key during a call attempt or during a call.

- Key depression does not affect ongoing calls or conversations.

#### To retransmit saved number

1. Press pre-programmed Save/Redial-key when telephone is idle.

System seizes Line 1 or Inquiry and then selects free trunk by stored digits can be sent.

### ECONOMYplus- and STANDARD Telephones

#### Save number

An extension saves a dialled number as follows:

1. Press 2nd-key.
2. Press Save/Redial during a call attempt or during a call.

- Key depression does not affect ongoing calls or conversations.

#### To retransmit saved number

1. Press 2nd-key.
2. Press Save/Redial when telephone is idle.

- System seizes Line 1, Line 2 or Inquiry and then selects free trunk by stored digits can be sent.

A telephone with display shows the transmitted digits.

### EXECUTIVE Telephones

#### Save number

An extension saves a dialled number as follows:

1. Press Menu-key Save (see display) during a call attempt or during a call.

- Key depression does not affect ongoing calls or conversations

#### To retransmit saved number

1. Press Menu-key Redial (see display) when telephone is idle.

- System seizes Line 1, Line 2 or Inquiry and then selects free trunk by stored digits can be sent.

The display shows the transmitted digits.

## Capacity

Each extension can save one external number with a maximum of 24 digits including intermediate tone(s) (if any) and area code.

## Limitations

Extensions equipped with Analogue telephones cannot save numbers.

A saved number is stored until a new number is stored.

If the number has been saved for a call via an external line key, retransmission takes place automatically via this external line key.

If the trunk line is busy on this occasion, a busy message will be supplied.

Retransmission of a saved number can only be activated from idle, internal or external register (dialling) state.

A saved number is coupled to the telephone and cannot be activated from the answering position in the case of activated follow me or diversion.

Nor can a saved number be accessed if the telephone has be locked by the user with the authorisation code

Save/Redial can be pressed at any time during an ongoing call and also afterwards.

Dial tones must be marked out during number dialling by depression of Mute so that the system waits for these tones upon retransmission.

## Programming

0301 |  | Key function

Enter function code = 37

## Equipment

System Telephones.

Revision: D © Ericsson Enterprise 2003