BusinessPhone Communication Platform 4.0
Commands > Commands 5000...5999

## 5212
Transfer allowed ?

This command determines whether transfer of calls is allowed to the number defined for system access. See command 5621 Define System access.

(To prohibit all calls to the system access number, erase this number.)

(System access from the system’s V.24 ports can be prevented by entering command 6012 Route on request.)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003