BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2081
Modified business key layout

This command defines whether or not the system should by default use the modified business key layout on DBC 2x1, 2x2 or 2x3 telephones. In the modified layout the transfer key is found on the first layer. Therefore, the diversion key is moved to the second layer.

Valid values: YES / NO

Default value: YES

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003