BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2342
Traffic check at call pick-up

This command states how the traffic group check should be executed for -

- individual call pickup
- group call pickup
- common call pickup

Alternatives:

0 = |  | Always allowed, no traffic group control.

1 = |  | The traffic group has to be open in at least one direction between the parties.

2 = |  | The traffic group has to be open in both directions between the parties.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003