BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8004
Hotel answering position

In the following traffic cases calls are re-routed to an answering position in the hotel:

- unanswered wake-up calls
- outgoing calls from barred guest extensions
- room-to-room calls, if barred

This command is used to determine to which answering position rewriting shall take place.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003