BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2078
Second central answering positon

The command is used to determine the 2nd (of 3) central answer position for the system in a corporate network. The programmable numbers can either be,

1-8 |  | CN reroute number when the answer position is located in other PBX. The programmed number must be the complete unique network number.

1-4 |  | Internal directory number when the answer position is located within the system. The call handling will be as for local rerouting, see further command 1104 Reroute position at night.

Value ‘blank’, 1-8 digit number.s

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003