BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1317
Complete called party number length

This command states the total amount of digits in called party number which is required before a call setup/seizure is started to the network. The digit dialling is supervised with register timer in accordance to command 1403 Time supervision of short register sign. alt. MFC/MFE outgoing. If the timer elapses then the call-setup is started without any further number length control.

Value = 1-32

not programmed = blank (ordinary called number handling)

In case of CN calls the C-NL category for private network router (commands 9115 Complete called party NL 1, 9125 Complete called party NL 2, 9135 Complete called party NL 3, 9145 Complete called party NL 4) overrides this trunk category.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003