BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1955
MCID activation request allowed from TEs ?

This command states whether MCID (Malicious Call Identification) is allowed by the terminal user(s) on the interface. A MCID request from terminal user is controlled before being sent to the T-interface.

Valid data:

No |  | MCID is not allowed

Yes |  | MCID is allowed

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003