BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1614
Call meter (CML) receiver level

The command is valid for call meter receiver CM 12/16 (with CML circuit ROA 219 5135/1). This command states the minimum level for the recognition of call-metering pulses.

Value = -20.0--45.0 dBm0 in steps of 0.5 dB

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003