BusinessPhone Communication Platform 4.0
Commands > Commands 7000...7999

## 7507
Max traffic limit timer

States the minimum number of free data timers that must exist in the system, so that extensions will not be kept blocked (cannot call the exchange). Value 0-255 free timers.

As soon as there are free timers, the blocking will stop. Ongoing and incoming calls are not affected by this blocking.

The limit is there to ensure that at peak periods, there will be enough CPU-resources for the traffic already ongoing in the exchange.

See also command 7506 High traffic limit timer.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003