BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1405
Wait time before metering is stopped

This command states for how long the call meter receiver will remain active after the release of the trunk.

The time is stated in 100 ms.

Value = 000-255 (0-25.5 s)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003