BusinessPhone Communication Platform 4.0
Dialogs

## Extension Gateway Administration Table

This table shows the following information about the IP extension gateway:

- # GW

- Number of the gateway

- IP address

- A unique, 32-bit number for a specific TCP/IP host on the Internet. Usually printed in decimal form (for example, 128.122.40.227).

- Q.931 port

- ITU-T standard. Describes call signalling.

- RAS port

- ITU-T standard. Describes call signalling.

- Status and ID

- The current status of the gateway extension and its ID.

#### Actions

Back |  | To return to the Gatekeeper Data dialog. |
Reload |  | To retrieve the current system settings. |

Revision: A © Ericsson Enterprise 2003