BusinessPhone Communication Platform 4.0
Commands > Commands 6000...6999

## 6009
Baud rate

The command defines the bit speed for the V24 port on the stated EXU- or CMU- board (ASB 150 01) respectively CPU-Dx or AUXx boards (ASB 150 02) for the local connection of a terminal, computer or printer.

For the type of the local-connected unit and the set of characters for the local-connected unit, the commands 6006 Device type, 6007 Character set and 6010 Master/Slave must be defined.

The following values are possible on the different types of peripheral boards, equipped with a V24 interface:

### IOU (except CPU-D4)

0 = |  | The stated board will not permit a local V24 connection

1 = |  | 50 Baud

2 = |  | 75 Baud

3 = |  | 110 Baud

4 = |  | 135 Baud

5 = |  | 150 Baud

6 = |  | 300 Baud

7 = |  | 600 Baud

8 = |  | 1200 Baud

9 = |  | 1800 Baud

10 = |  | 2400 Baud

11 = |  | *

12 = |  | 4800 Baud

13 = |  | 7200 Baud

14 = |  | 9600 Baud

### IOU (CPU-D4)

0 = |  | The stated board will not permit a local V24 connection

1 = |  | *

2 = |  | *

3 = |  | *

4 = |  | *

5 = |  | *

6 = |  | 300 Baud

7 = |  | 600 Baud

8 = |  | 1200 Baud

9 = |  | 1800 Baud

10 = |  | 2400 Baud

11 = |  | 3600 Baud

12 = |  | 4800 Baud

13 = |  | 7200 Baud

14 = |  | 9600 Baud

15 = |  | *

16 = |  | 19200 Baud

### SMU (except CPU-D4)

0 = |  | The stated board will not permit a local V24 connection

1 = |  | *

2 = |  | *

3 = |  | *

4 = |  | *

5 = |  | *

6 = |  | *

7 = |  | 600 Baud

8 = |  | 1200 Baud

9 = |  | *

10 = |  | *

### SMU (CPU-D4)

0 = |  | The stated board will not permit a local V24 connection

1 = |  | *

2 = |  | *

3 = |  | *

4 = |  | *

5 = |  | *

6 = |  | 300 Baud

7 = |  | 600 Baud

8 = |  | 1200 Baud

9 = |  | 1800 Baud

10 = |  | 2400 Baud

11 = |  | 3600 Baud

12 = |  | 4800 Baud

*) All bit speeds marked with a * are not supported on the appropriate peripheral board.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003