BusinessPhone Communication Platform 4.0
Commands > Commands 3000...3999

## 3601
Music source directory number

Sources for music-on-hold or background music are connected either to trunks reserved for this purpose or the analogue port on the CPU-D board. This command defines a link between a music source and a call number. If the music-source is the analog port on the CPU-D board, the call number is D#00.

If no link is defined, a parking tone is supplied instead of music.

Removal of a music source is done by pressing the dial key to erase the call number.

Before this command can be used, the commands for background music (5404 Create background music) or music-on-hold (5403 Create music on hold) must have been initiated. The trunk used for music shall be programmed for “no transmission” (command: 1302 Outgoing digit transmission) and “no PTS signal from parent exchange” (command: 1307 PTS-signal from parent exchange ?).

Range of values:

0-9999 |  | For trunk lines

D#00 |  | The analog input on the CPU-D board

D420-D42F |  | for announcement group (music-on-hold only)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003