BusinessPhone Communication Platform 4.0
Dialogs

## Trunk Copy Selection

In this dialog you can select one or more target trunk(s) that should obtain the same settings as the current trunk.

The Trunk Copy Selection dialog is displayed whenever you click on a Copy button in one of the Trunk Parameter dialogs. To access the copy selection, open a trunk list (analogue, CAS, ISDN, or IP) by selecting the “List trunks” option in the respective context menu. Then click on a trunk number in the table and click on the Copy button.

The following targets for copying are available:

- Copy to trunks on the same card
- Copy to all analogue trunks
- Copy to all CAS trunks
- Copy to all ISDN trunks
- Copy to all ISDN BA trunks
- Copy to all ISDN PRA trunks
- Copy to all IP trunks
- Copy to all trunks
- Copy to individual trunks
- Copy to individual extensions

### Copying of settings to trunks of the same type

- Click in one of the radio buttons in the Copy selection area to select the kind of target trunk.
- Click on the Submit button.

Note

If no command has been selected in the Trunk Parameter dialog, you are asked to select a command first.

- Click on the Close button to return to the Trunk Parameter dialog.

### Individual Trunk Selection

If you select the individual trunk option, you will automatically go to the bottom of the dialog to specify the target trunk(s).

Note

A parameter is copied to a target trunk only if the parameter is valid for this kind of trunk. Otherwise, the parameter will not be copied.

There are four ways to select a trunk directory number or a trunk directory range:

- Select the Directory Number from the drop-down list box and click on the Select trunk link on the right.
- Enter a Directory Range in the two fields and click on Select trunks link on the right. The range must consist of a trunk number sequence, e.g. 701-703.
- Check the box “(Un)Select all trunks”. This is a toggle box: If no trunk in the list below has been checked, you can select all trunks with just one click. If all trunks in the list below are checked, click in the check box to deselect all trunks.
- Check all target trunks manually in extension list.

Note

To deselect a trunk, just uncheck the respective check box.

- If you are satisfied with your changes, click on the Submit button. Now the settings are copied to the selected trunks.

Note

If no command has been selected in the Trunk Parameter dialog, you are asked to select a command first.

- Click on the Close button to return to the Trunk Parameter dialog.

#### Actions

Submit |  | To copy the settings to selected extensions. |
Reload |  | To reload the dialog and discard all changes. |
Detail |  | To view the trunk’s directory name and the I/F-Value of the trunk list. |
Sort by DirNum |  | To sort by directory number. |
Sort by Card/Ind |  | To sort by card & extension type. |
Close |  | To close the Extension Copy Selection and to return to the Trunk Parameter dialog. |

Revision: A © Ericsson Enterprise 2003