BusinessPhone Communication Platform 4.0
Commands > Commands 9000...9999

## 9133
Predigits choice 3

This command is used to define predigits, if any, for the 3-rd route choice.

The predigits are transmitted after the private network access code and before the dialled external number.

Predigits = 1 - 16.

Following commands for the 2-nd route choice will be ignored:

- 3302 Callback allowed?
- 3303 Predigits
- 3304 First alternative route
- 3305 Predigits for first alternative route
- 3306 Second alternative route
- 3307 Predigits for second alternative route

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003