BusinessPhone Communication Platform 4.0
Dialogs

## Trunk Parameter

Note

The trunk parameters depend on the trunk type and the trunk assignment.

Some parameters cannot be entered and are not displayed for analog trunks; the same applies for digital trunks and ISDN trunks. For ISDN trunks, the interface type assignment affects also the presence of trunk parameters. Only relevant parameters for the selected trunk type are shown in the dialog. This also results in different Index Bars in the Menu View above the trunk parameter dialog.

See facility description Trunk (486/15534-ASB 150 02 Uen).

In general, the dialog shows the following sections:

#### General

5605 |  | Directory number

6501 |  | Directory name

#### Call Handling

1001 |  | Facility COS

1003 |  | TCD-day COS

1004 |  | TCD-night COS

1005 |  | Common abbreviated number COS

1002 |  | Traffic number

1029 |  | Tenant group

1019 |  | Night-switching group

1030 |  | Public number group

1006 |  | Call back allowed?

1007 |  | Break-in allowed?

1008 |  | Camp-on to answering position?

1020 |  | Pick up parked trunk?

1018 |  | Subsystem to PBX

1023 |  | Trunk line type

1014 |  | Result tones to parent exchange?

1406 |  | Wait time before ring back/rerouting at not answered calls

1407 |  | Maximum hold time

1408 |  | Minimum speech time for not increasing disturbance counter

1409 |  | Time for recall on transfer before answer

1410 |  | Time fore recall on camp on

#### Outgoing Traffic Parameters

1013 |  | Dial tone to extension?

1034 |  | Public dial tone to extension?

1015 |  | Pre-digits for number analysis

1028 |  | LCR analysis required?

1036 |  | Type of IBERCOM network connection

1423 |  | Time supervision of B-answer

#### Incoming Traffic Parameters

1022 |  | Voice info to trunk allowed?

1031 |  | Answer by external line key allowed?

1101 |  | Answering position at day

1102 |  | Answering position at night

1105 |  | Common voice announcement at day

1106 |  | Common voice announcement at night

1107 |  | Busy voice announcement at day

1108 |  | Busy voice announcement at night

1109 |  | Common announcement interruptable

1039 |  | Multiple Music on Hold source number

1801 |  | Common number at automatic outgoing/incoming traffic

1802 |  | Pre-digits at automatic incoming traffic

1804 |  | DDI number translation

1103 |  | Reroute position at day

1104 |  | Reroute position at night

1009 |  | Reroute on answering position barred?

1010 |  | Reroute on answering position blocked?

1011 |  | Reroute on answering position vacant?

1012 |  | Reroute on answering position busy?

1016 |  | Reroute on no answer?

1017 |  | Reroute on incomplete number?

1411 |  | Time supervision for first digit at automatic incoming traffic

1412 |  | Time supervision between digits at automatic incoming traffic

1413 |  | Time supervision of answer at automatic incoming traffic

#### Register Signal Parameters

1307 |  | PTS-signal from parent exchange?

1308 |  | PTS-signal from parent exchange = dial tone

1309 |  | PTS-signal to parent exchange = dial tone?

1314 |  | Type of dial tone receiver, TRC

1317 |  | Complete called party number length

1401 |  | Number of digits with long dial supervision

1402 |  | Time supervision of long register sign. alt. MFC/MFE outgoing

1403 |  | Time supervision of short register sign. alt. MFC/MFE outgoing

1414 |  | Length detection first PTS

1415 |  | Length detection second PTS

#### Metering Parameters

1502 |  | Tariff number

1503 |  | Carrier number

#### Transmission parameters

1601 |  | CEPT-DTMF tone receiver level

1602 |  | ETOE-DTMF tone receiver level

1603 |  | Dial tone receiver level

1612 |  | Transmission group

#### Call information logging

6301 |  | Log outgoing calls?

6302 |  | Log duration time

6303 |  | Log minimum meter pulses

6304 |  | Bar outgoing calls?

6305 |  | Dialed number: suppress

6306 |  | Log dialed numbers beginning with 0

6307 |  | Log dialed numbers beginning with 1

6308 |  | Log dialed numbers beginning with 2

6309 |  | Log dialed numbers beginning with 3

6310 |  | Log dialed numbers beginning with 4

6311 |  | Log dialed numbers beginning with 5

6312 |  | Log dialed numbers beginning with 6

6313 |  | Log dialed numbers beginning with 7

6314 |  | Log dialed numbers beginning with 8

6315 |  | Log dialed numbers beginning with 9

6316 |  | Account code required for COS 0

6317 |  | Account code required for COS 1

6318 |  | Account code required for COS 2

6319 |  | Account code required for COS 3

6320 |  | Account code required for COS 4

6321 |  | Account code required for COS 5

6322 |  | Account code required for COS 6

6323 |  | Account code required for COS 7

6324 |  | Account code required for COS 8

6325 |  | Account code required for COS 9

6326 |  | Account code required for COS 10

6327 |  | Account code required for COS 11

6328 |  | Account code required for COS 12

6329 |  | Account code required for COS 13

6330 |  | Account code required for COS 14

6331 |  | Account code required for COS 15

6332 |  | Log minimum cost

#### Corporate network

1035 |  | Traveling class mark (TCM)

1037 |  | PNR routes at incoming proprietary call

1038 |  | Forward CLI/COL

1110 |  | 1st choice CN reroute position

1111 |  | 2nd choice CN reroute position

1112 |  | 3rd choice CN reroute position

A trunk can be selected for configuration by entering/selecting a directory number in the navigation section on top of the dialog.

5605 |  | Extension directory number

A link can be selected for configuration by entering/selecting a link number in the navigation section above the dialog.

Command | Value
– | Link Number | Existing link number 5 digits (0-9)

Input parameters can be marked (selected) via corresponding check boxes if appropriate. These selected parameters are then considered when the user wants to copy trunk data to other destination trunks. The (Un)select commands check box above the page can be used to (un)select all of the trunk parameters.

– | (Un)selected commands | Y/N (toggle)

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To load the current system settings. |
Copy |  | To access the dialog for copying parameters to other trunks. |

See facility description Trunk (486/15534-ASB 150 02 Uen).

Revision: A © Ericsson Enterprise 2003